{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Component List","Overview List"],"not_rendered":{"external_links":1,"defined_names":4},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Component List","index":0,"n_rows":85,"n_cols":10,"rows_kept":85,"merged":[[81,1,81,2]],"flags":["formulas_cached_only"]}
[]
[null,null,"Component List","ZKL3000 Switch Board"]
[null,null,"Source Data From:","me-zklswitch-board.PrjPCB"]
[null,null,"Project Name:","ZKL3000 Switch Board"]
[null,null,"Projectcode:","me-zkl3001switch-board"]
[null,null,"Report Date:","09-02-2017"]
[null,null,"Report Time:","11:49:00"]
[]
[null,"#","ComponentName","ComponentPackage","Manufacturer","ManufacturerNumber","Designator","Quantity","Quote","Replacement possible"]
[null,1,"22pF/0402","0402","AVX Corporation","04025A220KAT2A","C1, C2, C11, C12, C21, C22",6]
[null,2,"100nF-16V/0402","0402","AVX Corporation","0402YC104KAT2A","C3, C4, C5, C6, C7, C8, C10, C13, C14, C15, C16, C17, C18, C20, C23, C24, C25, C26, C27, C28, C30, C37, C47, C71",24]
[null,3,"4.7uF-16V/0402","0402","AVX Corporation","0402YD473KAT2A","C9, C19, C29",3]
[null,4,"10uF-25V/0805","0805","AVX Corporation","08053D106KAT2A","C31, C35",2]
[null,5,"22uF/1206","1206","AVX Corporation","12063D226KAT2A","C32",1]
[null,6,"100nF-25V/0402","0402","AVX Corporation","04023C104KAT2A","C33, C65_U_SwitchPower1, C65_U_SwitchPower2, C65_U_SwitchPower3, C65_U_SwitchPower4",5]
[null,7,"22uF/0402","0402","AVX Corporation","04026D226MAT2A","C34",1]
[null,8,"3.3nF/0402","0402","AVX Corporation","04025C332JAT2A","C36",1]
[null,9,"100pF/0402","0402","AVX Corporation","04025C101KAT2A","C38",1]
[null,10,"4700pF/0402","0402","AVX Corporation","04023C472KAT2A","C39, C43, C44",3]
[null,11,"470pF/0402","0402","AVX Corporation","04025C471KAT2A","C40",1]
[null,12,"0.22uF/0402","0402","AVX Corporation","0402ZD224KAT2A","C41, C45, C46, C54, C55, C69, C70, C78, C79",9]
[null,13,"10nF/0402","0402","AVX Corporation","04025C103KAT2A","C42, C48, C49, C56, C57, C72, C73, C81, C82",9]
[null,14,"1uF-10V/0402","0402","AVX Corporation","0402ZD105KAT2A","C50, C51, C52, C53, C58, C59, C60, C61, C74, C75, C76, C77, C83, C84, C85, C86",16]
[null,15,"OPEN/0402","0402","Meuleman Electronics","none","C62_U_SwitchPower1, C62_U_SwitchPower2, C62_U_SwitchPower3, C62_U_SwitchPower4",4]
[null,16,"0.022uF/2220","2220","Murata Electronics North America","GA355DR7GB223KW01L","C63_U_SwitchPower1, C63_U_SwitchPower2, C63_U_SwitchPower3, C63_U_SwitchPower4, C64_U_SwitchPower1, C64_U_SwitchPower2, C64_U_SwitchPower3, C64_U_SwitchPower4",8]
[null,17,"470nF-10V/0402","0402","AVX Corporation","0402ZD474KAT2A","C66_U_SwitchPower1, C66_U_SwitchPower2, C66_U_SwitchPower3, C66_U_SwitchPower4",4]
[null,18,"100nF/0805","0805","AVX Corporation","08055C104KAT2A","C67_U_SwitchPower1, C67_U_SwitchPower2, C67_U_SwitchPower3, C67_U_SwitchPower4, C68_U_SwitchPower1, C68_U_SwitchPower2, C68_U_SwitchPower3, C68_U_SwitchPower4",8]
[null,19,"BAS85/DO-213AC","DO-213AC","NXP Semiconductors","BAS85,135","D1, D2, D3, D4, D5, D6, D7, D11, D12, D13, D22, D23, D24, D28, D29, D30, D34",17]
[null,20,"BAT54,215/SOT23","SOT23","NXP","BAT54,215","D8, D9, D14, D15, D25, D26, D31, D32",8]
[null,21,"BAT54A/SOT23","SOT23","ST Microelectronics","BAT54AFILM","D10, D16, D27, D33",4]
[null,22,"SMAJ5.0CA-DO214AC","DO214AC","Littlefuse","SMAJ5.0CA","D17_U_SwitchPower1, D17_U_SwitchPower2, D17_U_SwitchPower3, D17_U_SwitchPower4",4]
[null,23,"SMAJ24CA-DO214AC","DO214AC","Littlefuse","SMAJ24CA","D18_U_SwitchPower1, D18_U_SwitchPower2, D18_U_SwitchPower3, D18_U_SwitchPower4, D19_U_SwitchPower1, D19_U_SwitchPower2, D19_U_SwitchPower3, D19_U_SwitchPower4, D20_U_SwitchPower1, D20_U_SwitchPower2, D20_U_SwitchPower3, D20_U_SwitchPower4, D21_U_SwitchPower1, D21_U_SwitchPower2, D21_U_SwitchPower3, D21_U_SwitchPower4",16]
[null,24,"WE690367290676/WE690367290676","WE690367290676","Wurth Electronics","690367290676","J1",1]
[null,25,"WE690367291076/WE690367291076","WE690367291076","Wurth Electronics","690367291076","J2, J3",2]
[null,26,"HDR1X6/HDR1X6","HDR1X6","Tyco Electronics","826629-6","J4, J6, J8",3]
[null,27,"HDR2X5-1.27mm/HDR2X5-1.27mm","HDR2X5-1.27mm","Wurth Electronics","62201021121","J5, J7, J9",3]
[null,28,"TSM-102-01-S-DV-P-TR/TSM-102-01-S-DV-P-TR","TSM-102-01-S-DV-P-TR","Samtec Inc","TSM-102-01-S-DV-P-TR","J10, J11, J14, J15, J16",5]
[null,29,"1KOHM/0805","0805","Wurth Elektronik","742792096","L1, L2, L3",3]
[null,30,"2.2uH/XFL4020","XFL4020","Coilcraft","XFL4020-222MEC","L4",1]
[null,31,"198.6µH/749196101","749196101","Wurth Elektronik","749196101","L5_U_SwitchPower1, L5_U_SwitchPower2, L5_U_SwitchPower3, L5_U_SwitchPower4, L6_U_SwitchPower1, L6_U_SwitchPower2, L6_U_SwitchPower3, L6_U_SwitchPower4",8]
[null,32,"120/0402","0402","Vishay Draloric","CRCW0402120RFKED","R1",1]
[null,33,"10K/0402","0402","Vishay Draloric","CRCW040210K0FKED","R2, R3, R6, R9, R12, R14, R16, R17, R20, R23, R26, R28, R30, R31, R34, R37, R40, R42, R49, R50, R53, R69, R75, R86, R92, R123, R129, R140, R146",29]
[null,34,"33/0402","0402","Vishay Draloric","CRCW040233R0FKED","R4, R7, R8, R11, R18, R21, R22, R25, R32, R35, R36, R39, R70, R76, R87, R93, R124, R130, R141, R147",20]
[null,35,"OPEN/0402","0402","Meuleman Electronics","none","R5, R10, R13, R15, R19, R24, R27, R29, R33, R38, R41, R43, R48, R67, R74, R84, R91, R105_U_SwitchPower1, R105_U_SwitchPower2, R105_U_SwitchPower3, R105_U_SwitchPower4, R106_U_SwitchPower1, R106_U_SwitchPower2, R106_U_SwitchPower3, R106_U_SwitchPower4, R121, R128, R138, R145",29]
[null,36,"18K/0402","0402","Vishay Draloric","TNPW040218K0BEED","R44",1]
[null,37,"100K/0402","0402","Vishay Draloric","CRCW0402100KFKED","R45, R64, R65, R73, R78, R90, R95, R127, R132, R144, R149",11]
[null,38,"7.5K/0402","0402","Vishay Draloric","CRCW04027K50FKED","R46",1]
[null,39,"2.4K/0402","0402","Vishay Draloric","CRCW04022K40FKED","R47",1]
[null,40,"10/0402","0402","Vishay Draloric","CRCW040210R0FKED","R51",1]
[null,41,"220/0402","0402","Vishay Draloric","CRCW0402220RFKED","R52, R79, R81, R96, R98, R133, R135, R150, R152",9]
[null,42,"220K/0402","0402","Vishay Draloric","CRCW0402220KFKED","R54, R56, R60, R61",4]
[null,43,"33K/0402","0402","Vishay Draloric","CRCW040233K0FKED","R55",1]
[null,44,"3.9K/0402","0402","Vishay Draloric","CRCW04023K90FKED","R57",1]
[null,45,"470/0402","0402","Vishay Draloric","CRCW0402470RFKED","R58, R72, R89, R126, R143",5]
[null,46,"1.8K/0402","0402","Vishay Draloric","CRCW04021K80FKED","R59",1]
[null,47,"100/0402","0402","Vishay Draloric","CRCW0402100RFKED","R62, R66, R68, R83, R85, R120, R122, R137, R139",9]
[null,48,"2.2K/0402","0402","Vishay Draloric","CRCW04022K20FKED","R63, R109_U_SwitchPower1, R109_U_SwitchPower2, R109_U_SwitchPower3, R109_U_SwitchPower4, R115_U_SwitchPower1, R115_U_SwitchPower2, R115_U_SwitchPower3, R115_U_SwitchPower4, R116_U_SwitchPower1, R116_U_SwitchPower2, R116_U_SwitchPower3, R116_U_SwitchPower4",13]
[null,49,"0/0402","0402","Vishay Draloric","CRCW04020000Z0ED","R71, R77, R88, R94, R103_U_SwitchPower1, R103_U_SwitchPower2, R103_U_SwitchPower3, R103_U_SwitchPower4, R104_U_SwitchPower1, R104_U_SwitchPower2, R104_U_SwitchPower3, R104_U_SwitchPower4, R125, R131, R142, R148",16]
[null,50,"820/0402","0402","Vishay Draloric","CRCW0402820RFKED","R80, R82, R97, R99, R112_U_SwitchPower1, R112_U_SwitchPower2, R112_U_SwitchPower3, R112_U_SwitchPower4, R134, R136, R151, R153",12]
[null,51,"470K/1206","1206","Vishay Draloric","TNPV1206470KBEEN","R100_U_SwitchPower1, R100_U_SwitchPower2, R100_U_SwitchPower3, R100_U_SwitchPower4, R101_U_SwitchPower1, R101_U_SwitchPower2, R101_U_SwitchPower3, R101_U_SwitchPower4, R102_U_SwitchPower1, R102_U_SwitchPower2, R102_U_SwitchPower3, R102_U_SwitchPower4",12]
[null,52,"2.4M/0402","0402","Vishay Draloric","CRCW04022M40JNED","R107_U_SwitchPower1, R107_U_SwitchPower2, R107_U_SwitchPower3, R107_U_SwitchPower4, R108_U_SwitchPower1, R108_U_SwitchPower2, R108_U_SwitchPower3, R108_U_SwitchPower4, R113_U_SwitchPower1, R113_U_SwitchPower2, R113_U_SwitchPower3, R113_U_SwitchPower4",12]
[null,53,"1M/0402","0402","Vishay Draloric","CRCW04021M00FKED","R110_U_SwitchPower1, R110_U_SwitchPower2, R110_U_SwitchPower3, R110_U_SwitchPower4",4]
[null,54,"15K/0402","0402","Vishay Draloric","CRCW040215K0FKED","R111_U_SwitchPower1, R111_U_SwitchPower2, R111_U_SwitchPower3, R111_U_SwitchPower4",4]
[null,55,"1.2M/0402","0402","Vishay Draloric","CRCW04021M20JNED","R114_U_SwitchPower1, R114_U_SwitchPower2, R114_U_SwitchPower3, R114_U_SwitchPower4",4]
[null,56,"82K/0402","0402","Vishay Draloric","CRCW040282K0FKED","R117_U_SwitchPower1, R117_U_SwitchPower2, R117_U_SwitchPower3, R117_U_SwitchPower4",4]
[null,57,"120K/0402","0402","Vishay Draloric","CRCW0402120KFKED","R118_U_SwitchPower1, R118_U_SwitchPower2, R118_U_SwitchPower3, R118_U_SwitchPower4",4]
[null,58,"4.7K/0402","0402","Vishay Draloric","CRCW04024K70FKED","R119_U_SwitchPower1, R119_U_SwitchPower2, R119_U_SwitchPower3, R119_U_SwitchPower4",4]
[null,59,"FDC6401N/TSOT-23-6","TSOT-23-6","Fairchild Semiconductor","FDC6401N","T1, T3, T4, T12, T13",5]
[null,60,"BSS308PE H6327/SOT23","SOT23","Infineon","BSS308PE H6327","T2",1]
[null,61,"IRFS4010PBF/D2PAK","D2PAK","Infineon","IRFS4010PBF","T5_U_SwitchPower1, T5_U_SwitchPower2, T5_U_SwitchPower3, T5_U_SwitchPower4, T6_U_SwitchPower1, T6_U_SwitchPower2, T6_U_SwitchPower3, T6_U_SwitchPower4, T7_U_SwitchPower1, T7_U_SwitchPower2, T7_U_SwitchPower3, T7_U_SwitchPower4, T8_U_SwitchPower1, T8_U_SwitchPower2, T8_U_SwitchPower3, T8_U_SwitchPower4, T10_U_SwitchPower1, T10_U_SwitchPower2, T10_U_SwitchPower3, T10_U_SwitchPower4, T11_U_SwitchPower1, T11_U_SwitchPower2, T11_U_SwitchPower3, T11_U_SwitchPower4",24]
[null,62,"FDG8850NZ/TSSOP6","TSSOP6","Fairchild Semiconductor","FDG8850NZ","T9_U_SwitchPower1, T9_U_SwitchPower2, T9_U_SwitchPower3, T9_U_SwitchPower4",4]
[null,63,"STM32F103CBT6/LQFP48","LQFP48","ST Microelectronics","STM32F103CBT6","U1, U3, U5",3]
[null,64,"SN65HVD230D/SOIC8","SOIC8","Texas Instruments","SN65HVD230D","U2, U4, U6",3]
[null,65,"LP2960IM-5.0/NOPB/SOIC16","SOIC16","Texas Instruments","LP2960IM-5.0/NOPB","U7",1]
[null,66,"TPS62140RGTR/VQFN16","VQFN16","Texas Instruments","TPS62140RGTR","U8",1]
[null,67,"AD8592ARMZ/MSOP10","MSOP10","Analog Devices","AD8592ARMZ-REEL","U9",1]
[null,68,"MCP604/SOIC14","SOIC14","Microchip","MCP604-I/SL","U10, U14",2]
[null,69,"LTC1540IS8/SOIC8","SOIC8","Linear Technology","ltc1540is8#pbf","U11_U_SwitchPower1, U11_U_SwitchPower2, U11_U_SwitchPower3, U11_U_SwitchPower4, U13_U_SwitchPower1, U13_U_SwitchPower2, U13_U_SwitchPower3, U13_U_SwitchPower4",8]
[null,70,"ILD205T/SOIC8","SOIC8","Vishay","ILD205T","U12_U_SwitchPower1, U12_U_SwitchPower2, U12_U_SwitchPower3, U12_U_SwitchPower4",4]
[null,71,"ABM3-8.000MHZ-D2Y-T/2-SMD","2-SMD","Abracon","ABM3-8.000MHZ-D2Y-T","X1, X2, X3",3]
[null,72]
[null,"Approved",null,null,"Notes"]
[]
[]
[{"$nulls":7}," "]

{"sheet":"Overview List","index":1,"n_rows":84,"n_cols":9,"rows_kept":84,"merged":[[80,1,80,2]],"flags":["formulas_cached_only"]}
[]
[null,null,"Overview List",null,"ZKL3000 Switch Board"]
[null,null,"Source Data From:",null,"me-zklswitch-board.PrjPCB"]
[null,null,"Project Name:",null,"ZKL3000 Switch Board"]
[null,null,"Projectcode:",null,"me-zkl3001switch-board"]
[null,null,"Report Date:",null,"09-02-2017"]
[null,null,"Report Time:",null,"11:49:00"]
[]
[null,"#","ComponentName","Manufacturer","ManufacturerNumber","Quantity"]
[null,1,"22pF/0402","AVX Corporation","04025A220KAT2A",6]
[null,2,"100nF-16V/0402","AVX Corporation","0402YC104KAT2A",24]
[null,3,"4.7uF-16V/0402","AVX Corporation","0402YD473KAT2A",3]
[null,4,"10uF-25V/0805","AVX Corporation","08053D106KAT2A",2]
[null,5,"22uF/1206","AVX Corporation","12063D226KAT2A",1]
[null,6,"100nF-25V/0402","AVX Corporation","04023C104KAT2A",5]
[null,7,"22uF/0402","AVX Corporation","04026D226MAT2A",1]
[null,8,"3.3nF/0402","AVX Corporation","04025C332JAT2A",1]
[null,9,"100pF/0402","AVX Corporation","04025C101KAT2A",1]
[null,10,"4700pF/0402","AVX Corporation","04023C472KAT2A",3]
[null,11,"470pF/0402","AVX Corporation","04025C471KAT2A",1]
[null,12,"0.22uF/0402","AVX Corporation","0402ZD224KAT2A",9]
[null,13,"10nF/0402","AVX Corporation","04025C103KAT2A",9]
[null,14,"1uF-10V/0402","AVX Corporation","0402ZD105KAT2A",16]
[null,15,"OPEN/0402","Meuleman Electronics","none",4]
[null,16,"0.022uF/2220","Murata Electronics North America","GA355DR7GB223KW01L",8]
[null,17,"470nF-10V/0402","AVX Corporation","0402ZD474KAT2A",4]
[null,18,"100nF/0805","AVX Corporation","08055C104KAT2A",8]
[null,19,"BAS85/DO-213AC","NXP Semiconductors","BAS85,135",17]
[null,20,"BAT54,215/SOT23","NXP","BAT54,215",8]
[null,21,"BAT54A/SOT23","ST Microelectronics","BAT54AFILM",4]
[null,22,"SMAJ5.0CA-DO214AC","Littlefuse","SMAJ5.0CA",4]
[null,23,"SMAJ24CA-DO214AC","Littlefuse","SMAJ24CA",16]
[null,24,"WE690367290676/WE690367290676","Wurth Electronics","690367290676",1]
[null,25,"WE690367291076/WE690367291076","Wurth Electronics","690367291076",2]
[null,26,"HDR1X6/HDR1X6","Tyco Electronics","826629-6",3]
[null,27,"HDR2X5-1.27mm/HDR2X5-1.27mm","Wurth Electronics","62201021121",3]
[null,28,"TSM-102-01-S-DV-P-TR/TSM-102-01-S-DV-P-TR","Samtec Inc","TSM-102-01-S-DV-P-TR",5]
[null,29,"1KOHM/0805","Wurth Elektronik","742792096",3]
[null,30,"2.2uH/XFL4020","Coilcraft","XFL4020-222MEC",1]
[null,31,"198.6µH/749196101","Wurth Elektronik","749196101",8]
[null,32,"120/0402","Vishay Draloric","CRCW0402120RFKED",1]
[null,33,"10K/0402","Vishay Draloric","CRCW040210K0FKED",29]
[null,34,"33/0402","Vishay Draloric","CRCW040233R0FKED",20]
[null,35,"OPEN/0402","Meuleman Electronics","none",29]
[null,36,"18K/0402","Vishay Draloric","TNPW040218K0BEED",1]
[null,37,"100K/0402","Vishay Draloric","CRCW0402100KFKED",11]
[null,38,"7.5K/0402","Vishay Draloric","CRCW04027K50FKED",1]
[null,39,"2.4K/0402","Vishay Draloric","CRCW04022K40FKED",1]
[null,40,"10/0402","Vishay Draloric","CRCW040210R0FKED",1]
[null,41,"220/0402","Vishay Draloric","CRCW0402220RFKED",9]
[null,42,"220K/0402","Vishay Draloric","CRCW0402220KFKED",4]
[null,43,"33K/0402","Vishay Draloric","CRCW040233K0FKED",1]
[null,44,"3.9K/0402","Vishay Draloric","CRCW04023K90FKED",1]
[null,45,"470/0402","Vishay Draloric","CRCW0402470RFKED",5]
[null,46,"1.8K/0402","Vishay Draloric","CRCW04021K80FKED",1]
[null,47,"100/0402","Vishay Draloric","CRCW0402100RFKED",9]
[null,48,"2.2K/0402","Vishay Draloric","CRCW04022K20FKED",13]
[null,49,"0/0402","Vishay Draloric","CRCW04020000Z0ED",16]
[null,50,"820/0402","Vishay Draloric","CRCW0402820RFKED",12]
[null,51,"470K/1206","Vishay Draloric","TNPV1206470KBEEN",12]
[null,52,"2.4M/0402","Vishay Draloric","CRCW04022M40JNED",12]
[null,53,"1M/0402","Vishay Draloric","CRCW04021M00FKED",4]
[null,54,"15K/0402","Vishay Draloric","CRCW040215K0FKED",4]
[null,55,"1.2M/0402","Vishay Draloric","CRCW04021M20JNED",4]
[null,56,"82K/0402","Vishay Draloric","CRCW040282K0FKED",4]
[null,57,"120K/0402","Vishay Draloric","CRCW0402120KFKED",4]
[null,58,"4.7K/0402","Vishay Draloric","CRCW04024K70FKED",4]
[null,59,"FDC6401N/TSOT-23-6","Fairchild Semiconductor","FDC6401N",5]
[null,60,"BSS308PE H6327/SOT23","Infineon","BSS308PE H6327",1]
[null,61,"IRFS4010PBF/D2PAK","Infineon","IRFS4010PBF",24]
[null,62,"FDG8850NZ/TSSOP6","Fairchild Semiconductor","FDG8850NZ",4]
[null,63,"STM32F103CBT6/LQFP48","ST Microelectronics","STM32F103CBT6",3]
[null,64,"SN65HVD230D/SOIC8","Texas Instruments","SN65HVD230D",3]
[null,65,"LP2960IM-5.0/NOPB/SOIC16","Texas Instruments","LP2960IM-5.0/NOPB",1]
[null,66,"TPS62140RGTR/VQFN16","Texas Instruments","TPS62140RGTR",1]
[null,67,"AD8592ARMZ/MSOP10","Analog Devices","AD8592ARMZ-REEL",1]
[null,68,"MCP604/SOIC14","Microchip","MCP604-I/SL",2]
[null,69,"LTC1540IS8/SOIC8","Linear Technology","ltc1540is8#pbf",8]
[null,70,"ILD205T/SOIC8","Vishay","ILD205T",4]
[null,71,"ABM3-8.000MHZ-D2Y-T/2-SMD","Abracon","ABM3-8.000MHZ-D2Y-T","3"]
[null,"Approved",null,null,"Notes"]
[]
[]
[{"$nulls":8}," "]